A screenshot of a phone

Description automatically generated with low confidence

# SG811 Sanitary Fixtures GUIDE NOTE: Refer to Design Guide sections DG / HYDRAULICS GENERALLY DG DRAINAGE (&TRADE WASTE)

|  |  |  |  |
| --- | --- | --- | --- |
| **ID** | **TITLE** | **COMPLIANCE LEVEL** |  |
|  |  |  |  |
| 1 | GENERAL |  | MANDATORY |
| *As per current* [*NATSPEC*](https://efsg.det.nsw.edu.au/user/login?destination=glossary#NATSPEC) *except as follows* | | | |
|  | | | |
| **1.0 General** | | | |
| In accordance with the **NSW Government Resource Efficiency Policy**, all fixtures and fittings must be at least the average [WELS](https://efsg.det.nsw.edu.au/glossary#WELS) star rating by product type. Where **WELS** rating is not available, use the alternative WaterMark rating scheme.  All new water-using appliances must be at least 0.5 stars above the average Water Efficiency Labelling and Standards (WELS) star rating by product type, except toilets and urinals, which must be purchased at the average **WELS** star rating.    Appliances and equipment purchased in the following categories with star ratings under the WELS scheme will be at least:     * showerheads – 3 stars (>7.5 but <=9.0 l/min) * toilets – 4 stars * urinals – 5 stars * dishwashers – 5 stars * taps and flow controllers – 5 stars. | | | |
|  | | | |
|  |  |  |  |
| 2 | PRODUCTS |  | MANDATORY |
| *As per current* [*NATSPEC 0811.2 Products*](https://efsg.det.nsw.edu.au/user/login?destination=glossary#NATSPEC) *except as follows* | | | |
|  | | | |
|  |  |  |  |
| 3 | EXECUTION |  | MANDATORY |
| *As per current* [*NATSPEC*](https://efsg.det.nsw.edu.au/user/login?destination=glossary#NATSPEC)  *0811.3 Execution.* | | | |
|  | | | |
|  |  |  |  |
| 4 | SELECTIONS |  | MANDATORY |
| *As per current* [*NATSPEC*](https://efsg.det.nsw.edu.au/user/login?destination=glossary#NATSPEC) *0811.4 elections except as follows* | | | |
|  | | | |
|  | | | |

**FIXTURE SCHEDULE**

# Basins schedule | Boys + Girls Communal Hall, Staff PS+HS, Materials Workshop HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Hs Materials Workshop  Ps Bulk Store (General Assistant)  Ps Hs Staff Toilets  Hs Toilets Boys + Girls (Gym Used as Entertainment Venue)  Ps Toilets Boys + Girls (Hall Used by Community) |
| **Catalogue Number**  **or Model** | [**105.32.10.01**](https://www.galvinengineering.com.au/galvinassist-type-c-500mm-wall-mount-basin-1-th-wi)  GalvinAssist® 500mm Wall Mount Basin, 1 TH with Overflow  **A white sink with a faucet  Description automatically generated with medium confidence** |
| **Material** | Vitreous China |
| **Colour** | White |
| **Size (L x W) (mm)** | 500 W X 410 L |
| **Tap Holes** | One (1) |
| **Soap Recesses** | Two (2) |
| **Trap + Shroud** | Concealed Trap + Shroud |
| **Bottle Traps** | Not Accepted |
| **Plug + Waste Outlet Size** | Complete With Anti Vandal Waste 40-32mm Chrome Plated Brass and White Plastic Plug |
| **Installation and Support** | Wall Mount Fixing Kit Included |
| **Overflow** | Yes |
| [**AS**](https://efsg.det.nsw.edu.au/glossary#AS)**Compliance** | AS 1428.1 |

# Basins schedule | Access (1 tap hole)

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS + PS Accessible Toilets  Accessible Bathrooms |
| **Catalogue Number**  **or Model** | [**105.32.10.01**](https://www.galvinengineering.com.au/galvinassist-type-c-500mm-wall-mount-basin-1-th-wi)  GalvinAssist® 500mm Wall Mount Basin, 1 TH with Overflow  **A white sink with a faucet  Description automatically generated with medium confidence** |
| **Material** | Vitreous China |
| **Colour** | White |
| **Size (L x W) (mm)** | 500 W X 410 L |
| **Tap Holes** | One (1) |
| **Soap Recesses** | Two (2) |
| **Trap + Shroud** | Concealed Trap + Shroud |
| **Bottle Traps** | Not Accepted |
| **Plug + Waste Outlet Size** | Complete With Anti Vandal Waste 40-32mm Chrome Plated Brass and White Plastic Plug |
| **Installation and Support** | Wall Mount Fixing Kit Included |
| **Overflow** | Yes |
| [**AS**](https://efsg.det.nsw.edu.au/glossary#AS)**Compliance** | AS 1428.1 |

# Basins schedule | Access (3 tap holes)

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS + PS Accessible Shower & Toilet  Assisted Shower  Toilet  Change Room |
| **CatalogueNumber**  **or Model** | **[105.32.10.03](https://www.galvinengineering.com.au/galvinassist-type-c-500mm-wall-mount-basin-3-th-wi)**  GalvinAssist® 500mm Wall Mount Basin, 3 TH with Overflow  **A white sink with a faucet  Description automatically generated with medium confidence** |
| **Material** | Vitreous China |
| **Colour** | White |
| **Size (L x W) (mm)** | 500 W X 410 L |
| **Tap Holes** | Three (3) |
| **Soap Recesses** | Two (2) |
| **Trap + Shroud** | Concealed Trap + Shroud |
| **Bottle Traps** | Not Accepted |
| **Plug + Waste Outlet Size** | Complete With Anti Vandal Waste 40-32mm Chrome Plated Brass and White Plastic Plug |
| **Installation and Support** | Wall Mount Fixing Kit Included |
| **Overflow** | Yes |
| [**AS**](https://efsg.det.nsw.edu.au/glossary#AS)**Compliance** | AS 1428.1 |

# Basins schedule | Individual Toilets, Clinic

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS + PS Staff  Staff Ambulant Toilets  Community Clinic |
| **Catalogue Number**  **or Model** | [**105.32.13.01**](https://www.galvinengineering.com.au/galvinassist-ultra-compact-wall-mount-basin-1-th-w)  GalvinAssist® Ultra-Compact, Wall Mount Basin, 1 TH with Overflow |
| **Material** | Vitreous China |
| **Colour** | White |
| **Size (L x W) (mm)** | 385 W X 250 L |
| **Tap Holes** | One (1) |
| **Soap Recesses** | Two (1) |
| **Trap + Shroud** | Concealed Trap + Shroud |
| **Bottle Traps** | Not Accepted |
| **Plug + Waste Outlet Size** | Complete With Anti Vandal Waste 40-32mm Chrome Plated Brass and White Plastic Plug |
| **Installation and Support** | Wall Mount Fixing Kit Included |
| **Overflow** | Yes |
| [**AS**](https://efsg.det.nsw.edu.au/glossary#AS)**Compliance** |  |

# Basins schedule | PS Staff Shower [SSP](https://efsg.det.nsw.edu.au/glossary#SSP)

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | PS Staff Shower |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Colour** |  |
| **Size (L x W) (mm)** |  |
| **Tap Holes** |  |
| **Soap Recesses** |  |
| **Trap + Shroud** |  |
| **Bottle Traps** |  |
| **Plug + Waste Outlet Size** |  |
| **Installation and Support** |  |
| **Overflow** |  |
| [**AS**](https://efsg.det.nsw.edu.au/glossary#AS)**Compliance** |  |

# Baths schedule | Senior Student Unit Toilet

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Senior Student Unit Toilet / Bathroom |
| **Catalogue Number**  **or Model** | **105.94.00.00  *(Coming Soon)***GalvinAssist® Slim Design Inwall Cistern, Less Flush Plate |
| **Material** | Acrylic |
| **Colour** | White |
| **Size (L x W) (mm)** | 1525 L X 720 W X 390 D |
| **Type** | Built In - Rectangular |
| **Wall Thickness (mm)** |  |
| **Waste Outlet Size** |  |
| **Installation and Support** |  |
| **Overflow** | Yes |
| **AS Compliance** |  |

# Sink schedule | Canteen

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS + PS Canteens |
| **Catalogue Number**  **or Model** | [**105.82.00.01**](https://www.galvinengineering.com.au/galvinassist-ss-150mm-sink-double-centre-bowls-1-t)  GalvinAssist® SS, 150mm Sink, Double Centre Bowls, 1 TH  A picture containing indoor, silver  Description automatically generated |
| **Material** | Stainless Steel  Grade 304, Bright Finish |
| **Bowls** | Two (2) |
| **Capacity Minimum** | 18 Litres (Each Bowl) |
| **Size (L x W) (mm)** | 350 W x 405 L x 180 D (Each Bowl) |
| **Drainer** | Twin Located Both Sides Of Bowls. Fluted Finish.  380mm Each Drainer |
| **Tap Holes** | One (1) |
| **Overflow** | Yes |
| **Overall Size** | 1500 L X 500 W |

# **Laundry Trough schedule | Laundry,** [GLS](https://efsg.det.nsw.edu.au/glossary#GLS) **(Art) Science Lab (eye wash), Visual Arts + Materials Workshop**

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Visual Arts Workshop  HS Materials Workshop |
| **Catalogue Number**  **or Model** | **105.83.10.01 *(Coming Soon)***  GalvinAssist® Free Standing Laundry Tub  A picture containing appliance  Description automatically generated |
| **Material** | Stainless Steel |
| **Bowls** | One (1) |
| **Capacity Minimum** | 45 Litre Bowls |
| **Overall Size (L x W) mm** | 600 W x 500 Lx 900 H |
| **Tap Holes** | One (1) |
| **Splashback Flange** | At Back 25mm H |
| **Bypass** | Yes |
| **Trough Mounting** | White Permacoat Steel Cabinet with Hinged Door |
| **Waste** | Stainless Steel Grate |
| **Splash Back** | Standard |
| **Splashback Material** | Stainless Steel Satin Finish |
| **Splashback Height** | 450 H |
| **Splashback Width** | Full Width of Laundry Trough |

# Bucket Sink schedule | hinged grate | Cleaners PS+HS, Botany/Zoology HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS + PS Cleaners Distributed Store Cleaning Supplies Store  HS Botany Store  *\* No vitreous china Bucket Sinks to be used on school projects* |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Finish** |  |
| **Overall Size** |  |
| **Back Flange** |  |
| **Overflow** |  |
| **Mounting** |  |
| **Mounting Height** |  |
| **Drainer** |  |
| **Hinged Grate Material** |  |

# Bucket Sink schedule | no hinged grate | Wood / metal workshop, Outdoor Covered Workshop HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Wood/Metal Workshop  Outdoor covered workshop *\* No vitreous china Bucket Sinks to be used on school projects* |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Finish** |  |
| **Overall Size** |  |
| **Overflow** |  |
| **Back Flange** |  |
| **Mounting** |  |
| **Mounting Height** |  |
| **Drainer** |  |

# Water Closet Assemblies | Access PS + HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS + PS Access Toilet Staff or Student  HS + PS Access Shower/Toilet  HS + PS Access Shower/ Toilet / Change |
| **Catalogue Number**  **or Model** | [**105.10.10.01**](https://www.galvinengineering.com.au/galvinassist-wall-faced-clean-flush-easy-care-acce~33656)  GalvinAssist® Wall Faced, Clean Flush, Easy Care, Accessible Toilet Suite with Blue Seat  A picture containing toilet  Description automatically generated |
| **WELS Rating** | 4 Star |
| **Dual Flush** | 4.5/ 3 Litre Dual Flush |
| **Backrest** | [**105.76.02.01**](https://www.galvinengineering.com.au/galvinassist-pwd-backrest)  GalvinAssist® PWD Backrest |
| **Seat** | Galvinassist® Single Flap Seat, Sorrento Blue, Institutional Hinges,  Rotatable/Buffers. Ensure Floor+ Wall Tile Colour Selection Achieves AS 1428.1 Luminous Contrast to Seat |
| **Material** | Vitreous China |
| **Cistern** | Complete With Integral Close Coupled Vitreous Cistern & Raised Buttons |
| **Cistern Buttons** | GalvinAssist® Raised Buttons |
| **Flush Pipe** |  |
| **As Compliance** | AS 1428.1 |

# Water Closet Assemblies Schedule | Girls Boys PS + HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | PS Toilets Boys + Girls  HS Toilets Boys + Girls |
| **Catalogue Number**  **or Model** | [**105.10.00.03**](https://www.galvinengineering.com.au/galvinassist-close-coupled-clean-flush-easy-care-t)  GalvinAssist® Close Coupled, Clean Flush, Easy Care, Toilet Suite, S-Trap, NSW EDU A picture containing toilet  Description automatically generated |
| **WELS Rating** | 4 Star |
| **Dual Flush** | 4.5/ 3 Litre Dual Flush |
| **Seat** | Blue Single Flap Vandal Resistant Seat and Blind Fixings |
| **Material** | Vitreous China |
| **Cistern** | GalvinAssist® Vitreous Cistern with Adjustable Height Connector 4.5/ 3 L Dual Flush, Wall Fixed Low Level Cistern |
| **AS Compliance** | AS 1172 |

# Water Closet Assemblies Schedule | Girls Boys Pre School + Early Childhood

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Pre school  Early Childhood Unit |
| **Catalogue Number**  **or Model** |  |
| **WELS Rating** |  |
| **Dual Flush** |  |
| **Height Floor to Seat** |  |
| **Seat** |  |
| **Material** |  |
| **Cistern** |  |
| **AS Compliance** |  |

# Water Closet Assemblies Schedule | Staff, Ambulant

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Staff  Staff + Student Ambulant |
| **Catalogue Number**  **or Model** | [**105.10.20.00**](https://www.galvinengineering.com.au/galvinassist-wall-faced-clean-flush-easy-care-ambu)  GalvinAssist® Wall Faced, Clean Flush, Easy Care, Ambulant Toilet Suite with Soft Close Seat  A white trash can  Description automatically generated with low confidence |
| **Dual Flush** | 4.5/ 3 Litre Dual Flush |
| **Seat** | Galvinassist® Single Flap Seat White |
| **Material** | Vitreous China |
| **Cistern** | Galvinassist® Integral Cistern 4.5/ 3 L Dual Flush, Wall Fixed Low-Level Cistern |
| **AS Compliance** | AS1428.1 |

# Urinal Assemblies Schedule | Boys PS + HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | PS + HS Toilets Boys |
| **Catalogue Number**  **or Model** |  |
| **Length** |  |
| **Fall to Centre Waste** |  |
| **Material** |  |
| **Outlet** |  |
| **Inlet** |  |
| **Anti-Drum Compound** |  |

# Urinal Flusher Schedule | Boys PS + HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | PS + HS Toilets Boys |
| **Catalogue Number**  **or Model** | [**TZ-FLOWFLUS**](https://www.galvinengineering.com.au/flowmatic-automatic-flusher-ceiling-wall-mounted-f) Flowmatic® Automatic Flusher Ceiling/Wall Mounted for Urinal 15 24v AC |
| **Type** | Flowmatic® Automatic Flusher Ceiling/Wall Mounted for Urinal 15 24v AC |
| **Solenoid Valve** | Solenoid Valve  AS MP52 Spec 030slow Shut Off to Reduce Water Hammer  Capable Of Operating in The Range of Varying Water Pressures Across NSW |
| **WELS** | 5 Star – When Installed on 600mm of Urinal |
| **Program Range** | Flush Duration: 5,10 Seconds  Flush Interval: 6,8,12,24 Hrs |
| **Reset** | Auto Reset to Programmed Operation After Power Failure |
| **Hygienic Flush** | One Flush Within A 12-Hr Period When Inactive. |
| **Power Supply** | 240 V Via AC Adaptor |
| **Installation** | Fully Concealed  Allow Access for Servicing |

# Fabricated SS Trough | Wash / Drinking Trough PS + HS

|  |  |  |  |
| --- | --- | --- | --- |
| **Property** | **Approved Product** | | |
| **Location** | Boys + Girls Toilets  Outdoor Learning Areas  Drinking Facilities General  HS Showers + Change | | |
| **Catalogue Number**  **or Model** |  | | |
| **Material** |  | | |
| **Outlet** |  | | |
| **Corners + Edging** |  | | |
| **Identification** |  | | |
| **Plumbing** |  | | |
| **Rim Height to Ground or FFL** |  | **Wash Trough** | **Drinking Trough** |
| **Pre School** |  |  |
| **Primary School** |  |  |
| **Secondary** |  |  |
| **Trough Guard** |  | | |
| **Splash Back** |  | | |
| **Support Assembly** |  | | |

# Fabricated SS Trough | Art Trough PS + HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Visual Arts Workshop  HS Materials Workshop  HS GLS with Art Space |
| **Catalogue Number**  **or Model** |  |
| **Type** |  |
| **Reference Drawing** |  |
| **Material** |  |
| **Size Type 1** |  |
| **Size Type 2** |  |
| **Outlet** |  |
| **Installation** |  |
| **Splash Back** |  |
| **Material** |  |

# Fabricated SS Trough | Special Art Trough with Bench  PS + HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | PS Outdoor Learning Area |
| **Reference** | Refer to EFSG / SG / SG DRAWING SG 504/1 |

# Clay / Plaster Arrestor | Art Trough with Pottery Wheel HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Visual Arts Workshop  GLS with Pottery Wheels |
| **Type 1** | Stainless Steel Clay/Plaster Arrestor with Removable Lid, Perforated Stainless Steel Strainer Basket and Baffles On Castors |
| **Reference Drawing** | SG / SG Drawing SG 405/2 |
| **Material** | Stainless Steel Grade 304  No4 Linish  0.9mm and 1.2 Mm Thick |
| **Connection** | 50mm Universal Trap |
| **Inlet** | PVC 50mm Diameter on Raised End of Unit |
| **Outlet** | PVC 50mm Diameter with Grate Removed |
| **Overflow** | Yes |
| **Strainer Basket** | Removable |
| **Perforations** | 2 mm Diameter  15 mm Centres |
| **Locating Springs** | Two (2) Attached to Baffle to Ensure Strainer Basket is Located Under Inlet Lip |
| **Baffles** | Two (2) Permanently Fixed |
| **Type 2** |  |
| **Removable** | One (1) Solid  One (1) Perforated |
| **Perforations** | 5 mm Diameter, 8 mm Centres |
| **Outlet Control** |  |
| **Type** | Box, Positioned Over Outlet with Open Bottom End and a 0.4 mm Diameter Hole in Top |
| **Maintenance** | Lid, Strainer Basket and Removable Baffles Must Be Able to be Removed while the Clay / Plaster Arrestor is in Position and without Disconnecting the Inlet and Outlet |

# Fabricated SS Trough | Plant Soaking Shelf Trough HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS |
| **Type** | Fabricated Flush SS Trough Assembly Recessed into Laminated Bench Top. Tapware with Anti-Rotation Lugs to be Fitted to Both Ends of The Tough |
| **Reference Drawing** | SG / SG Drawing SG 404/1  SG / SG Metalwork |
| **Material** | Stainless Steel Grade 304  Satin Finish  0.9 mm Thick |
| **Size** |  |
| **Height** | 950mm Rim Height from Floor |
| **Outlet** | 50mm, SS Grate with Sufficient Fall to Effectively Drain Water to the Grate, Locate in Centre |
| **Overflow** | Yes |
| **Splash Back** | Height 450 Mm from Top Of Benchtop  Fixed Securely to Wall |
| **Material** | Stainless Steel Grade 304  No4 Linish  0.9 mm Thick |

# Splashbacks | PS + HS

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Refer to EFSG / SG / MISCELLANEOUS FURNITURE /  STANDARD DoE FURNITURE ITEMS  Include List of Location/a where Splashbacks are Required |
| **Type** | Stainless Steel Splashback |
| **Material** | Stainless Steel Grade 304  No4 Linish  0.9 mm Thick |
| **Splash Back** | Height 450 mm from Top of Bench Unless Nominated Otherwise |
| **Length** | To Suit Application |
| **Installation** | Fix Securely to Wall. Seal Between Bottom Edge of Splashback and Benchtop with White Silicone Mastic, Gunned in, Waterproof Seal |

|  |  |  |  |
| --- | --- | --- | --- |
| **ID** | **TITLE** | **COMPLIANCE LEVEL** |  |
|  |  |  |  |
| 4.2 | SELECTIONS |  | MANDATORY |
| *As per current* [*NATSPEC*](https://efsg.det.nsw.edu.au/user/login?destination=glossary#NATSPEC) *0811.4 Selections except as follows* | | | |
|  | | | |
| *GUIDE NOTE:  Delete subclause "4.1 Sanitary Fixtures" nominated in NATSPEC Building Template/ Worksection and replace with the following text:* | | | |
| **4.1 Items with integrated Sanitary Fixtures Installed by Contractor – Refer SG / Miscellaneous Furniture Section**  All items to be installed by the building contractor in accordance with statutory requirements.  *GUIDE NOTE: Remove fixtures not required. Insert project specific locations.*  Refer to [EFSG](https://efsg.det.nsw.edu.au/glossary#EFSG) SG / MISCELLANEOUS FURNITURE. | | | |
|  | | | |

# B-05 Bench Cupboard  PS + HS | Staff, Sick Bay, First Aid, Library, [GLS](https://efsg.det.nsw.edu.au/glossary#GLS) | SK-42 sink

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Staff Room Adjoining Staff Annex  Sick Bay  Office Workroom  GLS with Sink  Library Administration |
| **Catalogue Number**  **or model** | **105.82.00.01**  GalvinAssist® SS, 1500mm Sink, Double Centre Bowls, 1 TH  *(3 TH also available)*  Text  Description automatically generated |
| **Material** | Stainless Steel  Grade 304, Bright Finish |
| **Bowls** | Two (2) |
| **Overflow** | Yes |
| **Capacity Minimum** | 18 Litre (Each Bowl) |
| **Size (L x W) (mm)** | 350 W x 420 L x 180 D (Each Bowl |
| **Drainer** | Twin Located Both Sides Of Bowls. Fluted Finish.  380mm Each Drainer |
| **Tap Holes** | One (1) *\*3 TH Also Available* |
| **Overall Size** | 1500 L X 500 W |

# B-06 Bench Cupboard HS | Science Learning Spaces | SK-32

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Science Learning Spaces |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Capacity Minimum** |  |
| **Size (L x W) (mm)** |  |
| **Tap Holes** |  |
| **Overall Size** |  |

# B-080S Bench Cupboard PS | PAA | SK-40

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Practical Activities Area  Shared Practical Activity Area  Practical Activities Area   io/is/p   [BD/CD/ED](https://efsg.det.nsw.edu.au/glossary#BDCDED)  Shared Practical Activity Area  [IO](https://efsg.det.nsw.edu.au/glossary#IO).[IS](https://efsg.det.nsw.edu.au/glossary#IS)/P   BD/CD/ED |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Size (L x W) (mm)** |  |
| **Tap Holes** |  |
| **Overall Size** |  |

# B-21 Bench Cupboard HS | PAA | SK-50

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Practical Activities Area |
| **Features** | B21 Bench Cupboard, Technology and Top, Bench Technology, SK 50 Craft Trough |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Size (L x W) (mm)** |  |
| **Tap Holes** |  |

# B-21 Bench Cupboard HS | Science Prep, Science GLS with Demonstration Bench | SK-32

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Science Preparation Area  HS GLS with Science Demonstration Bench |
| **Features** | B21 Bench Cupboard and Top, Bench Technology, SK32 Sink |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Capacity Minimum** |  |
| **Size (L x W) (mm)** |  |
| **Tap Holes** |  |
| **Overall Size** |  |

# B-21 Bench Cupboard HS | Staff, Community Clinic, Fitness Lab, Kitchen Type 1+2, GLS Type 7+14|SK-41

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Community Clinic & Staff Room  HS Clinic Boys  HS Fitness Laboratory  HS GLS Type 7 + 14  HS Preparation/Printing  HS Kitchen Type 1 and 2 |
| **Features** | B21 Bench Cupboard And Top, Bench Technology, Stainless Steel SK41 Sink |
| **Catalogue Number**  **or Model** | **105.82.00.01**  GalvinAssist® SS, 1500mm Sink, Double Centre Bowls, 1 TH  *(3 TH also available)*  Text  Description automatically generated |
| **Material** | Stainless Steel  Grade 304, Bright Finish |
| **Bowls** | Two (2) |
| **Capacity Minimum** | 18 Litre (Each Bowl) |
| **Size (L x W) (mm)** | 350 W x 420 L x 180 D (Each Bowl) |
| **Drainer** | Twin Located Both Sides Of Bowls. Fluted Finish.  380mm Each Drainer |
| **Tap Holes** | One (1) *\*3 TH Also Available* |
| **Overall Size** | 1200L x 500mm W x 180mm D |

# B-21 Bench Cupboard PS + HS | Sick Bay, Girls Clinic, Tea Room, Special Programs, Staff | SK-42

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Hs Clinic Girls  Tea Room  Special Programs Room  Staff Room  Ps Sick Bay |
| **Features** | B21 Bench Cupboard and Top, Bench Technology, Stainless Steel SK 42 Sink |
| **Catalogue Number**  **or Model** | **105.82.00.01**  GalvinAssist® SS, 1500mm Sink, Double Centre Bowls, 1 TH  *(3 TH also available)*  Text  Description automatically generated |
| **Material** | Stainless Steel  Grade 304, Bright Finish |
| **Bowls** | Two (2) |
| **Capacity Minimum** | 18 Litre (each bowl) |
| **Size (L x W) (mm)** | 350 W x 405 L x 180 D  each bowl |
| **Drainer** | Twin Located Both Sides of Bowls. Fluted Finish.  380mm Each Drainer |
| **Tap Holes** | Three (3) |
| **Overall Size** | 1500 L x 500 W |

# B-21 Bench Cupboard PS + HS | Support PAA, Tea Room, Kitchen Prep, Kitchen Type 1 + 2 | SK-34

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Practical Activities Area BD/CD/ED  Practical Activities Area [IO/IS/P](https://efsg.det.nsw.edu.au/glossary#IOISP)  Shared Practical Activities Area IO/IS/P  Tea Room  HS Kitchen Preparation  HS Kitchen Domestic and Semi-Commercial |
| **Features** | B21 Bench Cupboard and Top, Bench Technology, Stainless Steel SK34 Sink |
| **Catalogue Number**  **or Model** | **105.82.00.01**  GalvinAssist® SS, 1500mm Sink, Double Centre Bowls, 1 TH  *(3 TH also available)*  Text  Description automatically generated |
| **Material** | Stainless Steel  Grade 304, Bright Finish |
| **Bowls** | Two (2) |
| **Capacity Minimum** | 18 Litre (Each Bowl) |
| **Size (L x W) (mm)** | 350 W x 420 L x 180 D (Each Bowl) |
| **Drainer** | Twin Located Both Sides of Bowls. Fluted Finish.  380mm Each Drainer |
| **Tap Holes** | One (1) *\*3 TH Also Available* |
| **Overall Size** | 1200L x 500mm W x 180mm D |

# B-48 Bench Cupboard HS | Science Laboratory | SK-32

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Science Laboratory |
| **Features** | B48 Bench Demonstration Science |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Capacity Minimum** |  |
| **Size (L x W) (mm)** |  |
| **Tap Holes** |  |
| **Overall Size** |  |

# B-70 Darkroom Trough HS | Visual Art | SK-41

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Dark Room |
| **Features** | B70 Darkroom Trough with Bench Support T Aps, Trough and Tapware Supplied by the Nominated Furniture Supplier.  Installation, Install, Test and Commission all Fittings in Accordance with Statuary Requirements. |
| **Catalogue number or model** | **105.82.00.01**  GalvinAssist® SS, 1500mm Sink, Double Centre Bowls, 1 TH  *(3 TH also available)*  Text  Description automatically generated |
| **Material** | Stainless Steel  Grade 304, Bright Finish |
| **Bowls** | Two (2) |
| **Capacity minimum** | 18 Litre (Each Bowl) |
| **Size (L x W) (mm)** | 350 W x 420 L x 180 D (Each Bowl) |
| **Drainer** | Twin Located Both Sides of Bowls. Fluted Finish.  380mm Each Drainer |
| **Tap Holes** | One (1) *\*3 TH Also Available* |
| **Overall Size** | 1200L x 500mm W x 180mm D |

# M-79 Top PS| PAA | SK-40

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Practical Activities Area |
| **Features** | M-79 Top, Bench Technology, SK-40 (PA Trough) |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Size (L x W) (mm)** |  |
| **Tap Holes** |  |
| **Overall Size** |  |

# Sp-48 Bench Cupboard HS | Science | SK-32

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Science Laboratory |
| **Supply** | Sp-48 Bench, height adjustable (front wind), Science, flexible waste connection |
| **Catalogue Number**  **or Model** |  |
| **Material** |  |
| **Capacity Minimum** |  |
| **Size (L x W) (mm)** |  |
| **Tap Holes** |  |
| **Overall Size** |  |

# Sp-49 Bench Cupboard HS | Kitchen Type 1 | SK-41

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | HS Kitchen Domestic |
| **Supply** | Sp-49 Bench, Height Adjustable (Front Wind), Kitchen, Flexible Waste Connection |
| **Catalogue Number**  **or Model** | **105.82.00.01**  GalvinAssist® SS, 1500mm Sink, Double Centre Bowls, 1 TH  *(3 TH also available)*  Text  Description automatically generated |
| **Material** | Stainless Steel  Grade 304, Bright Finish |
| **Bowls** | Two (2) |
| **Capacity Minimum** | 18 Litre (Each Bowl) |
| **Size (L x W) (mm)** | 350 W x 420 L x 180 D (Each Bowl) |
| **Drainer** | Twin Located Both Sides of Bowls. Fluted Finish.  380mm Each Drainer |
| **Tap Holes** | One (1) *\*3 TH Also Available* |
| **Overall Size** | 1200L x 500mm W x 180mm D |

# B-0506 Bench Cupboard | Support PAA | SK-41

|  |  |
| --- | --- |
| **Property** | **Approved Product** |
| **Location** | Practical Activities Area BD/CD/ED |
| **Supply** | B-0506 Bench Cupboard 1200, Sink (white) |
| **Catalogue Number**  **or Model** | **105.82.00.01**  GalvinAssist® SS, 1500mm Sink, Double Centre Bowls, 1 TH  *(3 TH also available)*  Text  Description automatically generated |
| **Material** | Stainless Steel  Grade 304, Bright Finish |
| **Bowls** | Two (2) |
| **Capacity Minimum** | 18 Litre (Each Bowl) |
| **Size (L x W) (mm)** | 350 W x 420 L x 180 D (Each Bowl) |
| **Drainer** | Twin Located Both Sides of Bowls. Fluted Finish.  380mm Each Drainer |
| **Tap Holes** | One (1) *\*3 TH Also Available* |
| **Overall Size** | 1200L x 500mm W x 180mm D |